1	품 명	Echo Cancel DSP Mixer
	수량 및 단위	1대
□ 용도 : 에코캔슬 DSP 믹서 □ 기능 및 특징 ◎ 완전한 디지털 에코캔슬 오디오 매트릭스 및 믹서 ◎ 오디오 품질을 개선하도록 설계된 마이크로프로세서 제어 프로그래밍 가능 자동 믹서 ◎ 6개 밸런스 입력은 각각 전환 가능한 48볼트 팬텀 전원을 제공 ◎ 12대역 완전 파라메트릭 EQ, 컴프레서, 리미터 및 8대역 피드백 억제기가 장착 ◎ 믹서 전면 패널의 컨트롤 및 LED 표시기로 사용자가 쉽게 조정 ◎ 대규모 멀티 마이크 설치의 경우 최대 6개의 본체를 확장 연결하여 구성가능 □ 규격 • 4 balanced mic inputs, 2 balanced Mic/Line inputs and 1 stereo unbalanced input • 1 stereo and 2 mono outputs • 2-channel USB audio interface for soft codec integration or playback from computer • Onboard acoustic echo canceler (AEC) processing • Full digital processing on inputs and outputs • 8 x 3 audio routing matrix • 6-channel Digital Mixer (gate or gain sharing) • Front panel direct operation and Web Remote functionality • IP control for third-party CCS administration • Up to 6 Echo DSP mixers can be linked using Cat5e cable • Each output channel shall be equipped with adjustable output level, 12-band fully parametric EQ with notch filtering, compressor, limiter, and 8-band feedback suppressor. • Input Impedance : Mic: 1,600 ohms Line: 10,000 ohms ST (L/R): 10,000 ohms • Output Impedance : Balanced: 150 ohms Unbalanced: 150 ohms • Maximum Gain : 64 dB • Frequency Response : 20Hz to 20kHz (Mic -16dBu): ±1dB, (Mic -60dBu): +1/-2dB 20Hz to20 kHz (Line 24dBu): ±1dB, (Line -40dBu): +1/-2dB • Dynamic Range : 110 dB or higher, A-weighted/ST • Signal-to-noise ratio1 : 90 dB or higher, A-weighted/ST • Equivalent Input Noise : -126 dBu or less, Rs=150 ohms, DIN • Common-Mode Rejection Ratio : 80 dB or higher, 1 kHz • Residual Noise : -86 dBu or less, A-weighted • Channel Separation : -80 dB or less, 1 kHz unity • Total Harmonic Distortion : 0.03% or less, 1 kHz unity • Mic/Line Input Pads : -24 dB • Microphone Phantom Power : +48V DC □ 기타 (1) 제조자 공급확약서 (2) 전원 케이블 (3) Manual